To blank EGA/VGA screen - read flipflop at 0x3DA, then write 0x00
                          to control port at 0x3C0

To restore screen       - read flipflop at 0x3DA, then write 0x020
                          to control port at 0x3C0
