;---------------------------------------------------------------
; DISPLAY ADAPTER INFORMATION LOOKUP TABLE
;
; This is the lookup table containing information on all legal
; display adapters.  The first field in each element is a 26-
; character string containing a brief description of the
; adapter.  The next field is the segment of the video refresh
; buffer.  The last three fields are the number of screen lines
; an adapter displays when the 8-pixel, 14-pixel, and 16-pixel
; fonts are loaded, respectively.  Note that not all adapters
; support all fonts, but a screen line count is given for all
; three fonts for all adapter types.  Illegal combinations will
; not be accessed.
;---------------------------------------------------------------
VidInfoTbl DB      'No adapter identified      '    ; Code 0
           DW      0B000H
           DB      25,25,25
           DB      'Monochrome Display Adapter '    ; Code 1
           DW      0B000H
           DB      25,25,25
           DB      'Color Graphics Adapter     '    ; Code 2
           DW      0B800H
           DB      25,25,25
           DB      'Code 3: Undefined          '    ; Code 3
           DW      0B000H
           DB      25,25,25
           DB      'EGA with color monitor     '    ; Code 4
           DW      0B800H
           DB      43,25,25
           DB      'EGA with mono monitor      '    ; Code 5
           DW      0B000H
           DB      43,25,25
           DB      'Code 6: Undefined          '    ; Code 6
           DW      0B000H
           DB      25,25,25
           DB      'VGA with mono monitor      '    ; Code 7
           DW      0B000H
           DB      50,27,25
           DB      'VGA with color monitor     '    ; Code 8
           DW      0B800H
           DB      50,27,25
           DB      'Code 9: Undefined          '    ; Code 9
           DW      0B000H
           DB      25,25,25
           DB      'MCGA with digital color    '    ; Code 0AH
           DW      0B800H
           DB      25,25,25
           DB      'MCGA with monochrome       '    ; Code 0BH
           DW      0B000H
           DB      25,25,25
           DB      'MCGA with analog color     '    ; Code 0CH
           DW      0B800H
           DB      25,25,25
